NOW AVAILABLE!!

The latest firmware and software for the Max4 (v1.06). We have updated the limits to allow for 70A before the error is set and also updated some of the bugs associated with the 120A mode.

The link below contains a full installation of the software.

Max4 Software/Firmware v1.06


1.       Run ‘Setup’ to install the software
2.	 Once the software is installed and drivers have been installed open the Max 4 software and press "F12"
3.       Use the new version of the software to download v1.06 firmware to a Max4 unit 